help message : help
show version num : version
list PIDs of processes hosting a JDWP transport : jdwp

copy file/dir to device : push <local> <remote>
copy file/dir from device : pull <remote> [<local>]
copy host->device only if changed : sync [ <directory> ]
run remote shell command : shell <command>
run emulator console command : emu <command>
View device log : logcat [ <filter-spec> ]
forward socket connections : forward <local> <remote>
push a package to the device and install it : install [-l] [-r] [-s] <file>
remove a package from the device : uninstall [-k] <package>
return bug report : bugreport
block until device is online : wait-for-device
ensure that there is a server running : start-server
kill the server if it is running : kill-server
prints offline | bootloader | device : get-state
prints <serial-number> : get-serialno
remounts the /system partition on the device read-write : remount
reboots the device : reboot [bootloader|recovery]
reboots the device into the bootloader : reboot-bootloader
restarts the adbd daemon with root permissions : root
restarts the adbd daemon listening on USB : usb
restarts the adbd daemon listening on TCP port : tcpip <port>
Run PPP over USB. : ppp <tty> [parameters]


